| FRONT WIRING
H45/BVVR/2TR

#### 1337
SWITCHING PROTECTION UNIT
DG/TR4X2/SSESP/NINAV4/RAD04,RAD05,RAD07

1 | 0.5 | AP4 | PROTECTED + AFTER IGNITION AUTOMATIC TRANSMISSION FUSE | ?????
4 | 0.5 | 49BB | FAN CONTROL RELAY 2 | ?????
5 | 0.5 | 49BA | FAN CONTROL RELAY 1 | ?????
8 | 0.3 | A5 | ENGINE AFTER IGNITION CONTROL RELAY | ?????
11 | 0.3 | 67G | ELECTRIC CONTROL UNIT > AUDIBLE WARNING ACTIVATION SIGNAL | ?????