| ENGINE WIRING
2TR/BVVR

#### 120
INJECTION COMPUTER
CA01,CA02/2TR703

A1 | 0.5 | 3MO | MOTORISED THROTTLE POTENTIOMETER SENSOR - | ?????
B1 | 0.5 | 38U | RHEOSTAT CURSOR | ?????
E1 | 0.5 | 3JK | COOLANT TEMPERATURE - | ?????
F1 | 0.5 | 3DU | AIRFLOW SENSOR - | ?????
G1 | 0.5 | 3BL | ENGINE SPEED > TDC SENSOR - SIGNAL | ?????
H1 | 0.5 | 3SX | - INLET CAMSHAFT SENSOR | ?????
K1 | 0.5 | 38Y | REFRIGERANT GAS PRESSURE SENSOR + | ?????
L1 | 0.5 | 3ACN | TDC SENSOR/ENGINE SPEED + SIGNAL | ?????
A2 | 0.5 | 3GJ | DOWNSTREAM OXYGEN SENSOR EARTH | ?????
B2 | 0.5 | 38X | REFRIGERANT GAS PRESSURE SENSOR SIGNAL | ?????
D2 | 0.5 | 3MN | MOTORISED THROTTLE POTENTIOMETER + 5 VOLTS | ?????
G2 | 0.5 | 3QK | + CAMSHAFT SENSOR SIGNAL | ?????
J2 | 0.5 | 3DQ | PINKING SENSOR - | ?????
B3 | 0.5 | 3MQ | MOTORISED THROTTLE POTENTIOMETER 2 SIGNAL | ?????
D3 | 0.5 | 3C | COOLANT TEMPERATURE SENSOR + SIGNAL | ?????
E3 | 0.5 | 3DW | AIRFLOW SENSOR - SIGNAL | ?????
G3 | 0.5 | 3DV | AIRFLOW SENSOR + SIGNAL | ?????
M3 | 0.5 | 3SZ | VARIABLE INLET CAMSHAFT CONTROL | ?????
A4 | 0.5 | 3GL | DOWNSTREAM OXYGEN SENSOR SIGNAL | ?????
B4 | 0.5 | 3MP | MOTORISED THROTTLE POTENTIOMETER 1 SIGNAL | ?????
D4 | 0.5 | 3GK | UPSTREAM OXYGEN SENSOR SIGNAL | ?????
E4 | 0.5 | 3GH | UPSTREAM OXYGEN SENSOR EARTH | ?????
H4 | 0.5 | 3S | PINKING SENSOR 1 + SIGNAL > FRONT | ?????
J4 | 0.5 | 3BG | ENGINE SPEED SIGNAL > TDC SENSOR | ?????
K4 | 0.5 | 3SV | INLET CAMSHAFT SENSOR SIGNAL | ?????
M4 | 1.2 | AP15 | PROTECTED + AFTER IGNITION ENGINE FUNCTIONS FUSE | ?????