| CONNECTION
ANY TYPE

#### R455
DASHBOARD/LEFT REAR 5
H45/DG TR4X2/SOP03/RAD02,RAD04,RAD05

2 | 0.5 | 34A | LEFT HAND REAR LOUDSPEAKER + SIGNAL | ?????
3 | 1.2 | A1 | + AFTER IGNITION ELECTRIC WINDOW FUSE > RELAY | ?????
4 | 1.2 | 20AR | DEADLOCKING MOTOR CONTROL | ?????
5 | 1.2 | 20BD | OPEN FRONT/REAR PASSENGER DOORS MOTOR CONTROL | ?????
6 | 1.2 | 23K | LEFT HAND REAR ELECTRIC WINDOW CONTROL 2 | ?????
7 | 1.2 | 36A | REAR WIPER + CONTROL | ?????
9 | 0.5 | 34B | LEFT HAND REAR LOUDSPEAKER - SIGNAL | ?????
10 | 1.2 | 15LP | PROTECTED HEATED REAR SCREEN + CONTROL | ?????
11 | 1.2 | BP48 | PROTECTED + BATTERY FEED > ELECTRIC WINDOW | ?????
12 | 1.2 | A1 | + AFTER IGNITION ELECTRIC WINDOW FUSE > RELAY | ?????
13 | 1.2 | 20D | ELECTRIC DOOR LOCKS CLOSE + CONTROL | ?????
15 | 1.2 | BP48 | PROTECTED + BATTERY FEED > ELECTRIC WINDOW | ?????
16 | 1.2 | 23J | LEFT HAND REAR ELECTRIC WINDOW CONTROL 1 | ?????