| RIGHT-HAND REAR DOOR WIRING
H45

#### 201
REAR RIGHT-HAND WINDOW MOTOR
DG,DD/LVILVI/NINAV1/RAD02

13 | 1.2 | 21ZB | WINDOW WINDER THERMAL PROTECTION SIGNAL | C426E
14 | 1.2 | MZT | RIGHT-HAND REAR ELECTRIC EARTH ARRANGEMENT | C426E
5 | 1.2 | 23B | ELECTRIC WINDOW DOWN CONTROL > RIGHT HAND REAR QUARTER LIGHT OPEN | ?????
6 | 0.3 | 23X | REAR LEFT-HAND ANTI-PINCH WINDOW WINDER SERIES SIGNAL | F005E
7 | 1.2 | 23A | ELECTRIC WINDOW CONTROL > RIGHT-HAND REAR QUARTER LIGHT CLOSE | ?????
11 | 1.2 | 23AA | REAR RIGHT-HAND ELECTRIC WINDOW RAISE/LOWER CONTROL | ?????