| CONNECTION
ANY TYPE

#### R480
REAR LEFT-HAND WIRING / FRONT WIRING CONNECTION 2
H45/DD TR4X4/NINAV2/RAD03

1 | 0.85 | H66P | REVERSING LIGHTS + CONTROL | ?????
2 | 1.2 | 79A | HEATED SEAT + CONTROL | ?????
3 | 3.0 | 38JS | CONTROL 1 REAR DISTRIBUTION MOTOR | ?????
4 | 2.0 | BP89 | AUTOMATIC PARKING BRAKE FUSE PROTECTED + BATTERY FEED | ?????
5 | 0.5 | 79FA | HEATED SEAT WARNING LIGHT CONTROL, LOW POSITION | ?????
6 | 0.5 | 79FB | HEATED SEAT WARNING LIGHT CONTROL, HIGH POSITION | ?????