| CONNECTION
ANY TYPE

#### R2
DASHBOARD/LEFT REAR CONNECTION
H45/DD FMMANU,FPAUTO/RDAVAR/SOP01/RETRCR/LVILVE/RAD01,RAD02/BVM6

1 | 0.5 | 87T | BOOT LID POSITION SWITCH 1 SIGNAL | ?????
5 | 0.3 | 87A | LEFT HAND REAR 1st POSITION SWITCH - SIGNAL | ?????
6 | 0.3 | 87H | DRIVER'S 1st POSITION SWITCH - SIGNAL | ?????
8 | 0.3 | LP | PROTECTED + SIDE LIGHT FEED | ?????
9 | 0.5 | 151R | BUZZER + | ?????
10 | 0.5 | 35N | FRONT LOUDSPEAKER SIGNAL | ?????
11 | 0.3 | 70BS | LEFT-HAND REAR WHEEL AERIAL RECEIVER + SUPPLY | ?????
12 | 0.3 | 70BT | LEFT-HAND REAR WHEEL RADIO FREQUENCY AMPLITUDE SIGNAL | ?????
13 | 0.3 | 47F | VEHICLE SPEED SIGNAL | ?????
14 | 0.5 | BPT | PROTECTED + BATTERY FEED TIMER | ?????
15 | 0.5 | AP44 | POWER ASSISTED STEERING ECU + AFTER IGNITION FEED FUSE PROTECTION | ?????
16 | 0.5 | 85U | 4X4 SOLENOID VALVE - CONTROL | ?????
17 | 0.85 | 20S | TAILGATE MOTOR OPENING AUTHORISED FEED | ?????
18 | 0.5 | 20G | TAILGATE MOTOR OPEN CONTROL | ?????
25 | 0.5 | 151E | PARKING AID WARNING LIGHT CONTROL | ?????
26 | 0.5 | 151W | PARKING AID DEACTIVATION | ?????
27 | 0.3 | 70BV | LEFT-HAND REAR WHEEL AERIAL RECEIVER EARTH | ?????
28 | 0.3 | 70BU | LEFT-HAND REAR WHEEL AERIAL RECEIVER SIGNAL | ?????
29 | 0.5 | 60ES | FRONT RIGHT-HAND PRESENCE / POSITION EARTH | ?????
29 | 0.5 | 60ES | FRONT RIGHT-HAND PRESENCE / POSITION EARTH | ?????
30 | 0.5 | 13E | INTERIOR LIGHTS - CONTROL > TIMER | ?????
31 | 0.5 | 64C | LEFT HAND TURN SIGNAL LIGHTS CONTROL | ?????
32 | 0.5 | 85T | 4X4 SOLENOID VALVE + CONTROL | ?????