| ENGINE WIRING
2TR/BVM6

#### 1076
MOTORISED THROTTLE BODY
TR4X2,TR4X4/CA01,CA02/2TR700

1 | 0.85 | 3AJC | THROTTLE MOTOR - CONTROL | F005E
2 | 0.85 | 3AJB | THROTTLE MOTOR + CONTROL | F005E
3 | 0.5 | 3MO | MOTORISED THROTTLE POTENTIOMETER SENSOR - | F005E
4 | 0.5 | 3MQ | MOTORISED THROTTLE POTENTIOMETER 2 SIGNAL | F005E
5 | 0.5 | 3MP | MOTORISED THROTTLE POTENTIOMETER 1 SIGNAL | F005E
6 | 0.5 | 3MN | MOTORISED THROTTLE POTENTIOMETER + 5 VOLTS | F005E