| CONNECTION
ANY TYPE

#### R450
DASHBOARD/RIGHT REAR 3
H45/DD FPAUTO/RDAVAR/SOP03/RETRCR/LVILVI/NINAV2/BVM6

2 | 0.5 | 60EH | FRONT RIGHT-HAND SEAT BELT SWITCH SIGNAL | ?????
3 | 0.5 | 34MA | RADIO SOCKET AUXILIARY INPUT SIGNAL | ?????
4 | 0.3 | 70BM | RIGHT-HAND REAR WHEEL AERIAL RECEIVER + SUPPLY | ?????
5 | 0.3 | 70BP | RIGHT-HAND REAR RADIO FREQUENCY AMPLITUDE SIGNAL | ?????
6 | 0.3 | 26P | DOOR HANDLE INFRARED SENSOR + | ?????
7 | 0.3 | 26AM | KEYLESS VEHICLE BOOT LID EXTERNAL AERIAL A SIGNAL | ?????
8 | 0.3 | 26AK | KEYLESS VEHICLE REAR PASSENGER DOOR EXTERNAL AERIAL A SIGNAL | ?????
9 | 0.3 | 87B | RIGHT HAND REAR 1st POSITION SWITCH - SIGNAL | ?????
12 | 0.5 | 34MC | HEADPHONE AUXILIARY INPUT EARTH | ?????
13 | 0.5 | 34MB | RADIO SOCKET AUXILIARY INPUT SIGNAL | ?????
14 | 0.3 | 70BR | RIGHT-HAND REAR WHEEL AERIAL RECEIVER EARTH | ?????
15 | 0.3 | 70BQ | RIGHT-HAND REAR WHEEL AERIAL RECEIVER SIGNAL | ?????
16 | 0.3 | 26R | RIGHT HAND REAR HANDLE INFRARED SENSOR SIGNAL | ?????
17 | 0.3 | 26AN | KEYLESS VEHICLE BOOT LID EXTERNAL AERIAL SIGNAL2 | ?????
18 | 0.3 | 26CK | PASSENGER REAR DOOR SWITCH/LOCKING SIGNAL | ?????
19 | 0.3 | 26AL | KEYLESS VEHICLE REAR PASSENGER DOOR EXTERNAL AERIAL B SIGNAL | ?????
20 | 0.3 | 87G | PASSENGER'S 1st POSITION SWITCH - SIGNAL | ?????