| DASHBOARD WIRING
H45/DG

#### 645
PASSENGER COMPARTMENT COMPUTER
FMMANU/SOP01/LVILVE/NINAV1/BVM6

9 | 0.3 | 26BD | UCH SYNCHRONISATION / CARD READER SIGNAL | ?????
10 | 0.3 | 26BG | UCH DATA / CARD READER SIGNAL | ?????
11 | 0.3 | A4 | PASSENGER COMPARTMENT AFTER IGNITION CONTROL RELAY | ?????
12 | 0.3 | 26H | RADIO FREQUENCY SIGNAL | ?????
13 | 0.3 | 26BH | + CARD READER | ?????
14 | 0.3 | 67A | HORN + CONTROL | ?????
16 | 0.3 | 141P | INFORMATION DISPLAY STEERING WHEEL MOUNTED CONTROL COLUMN 5 SIGNAL | ?????
17 | 0.3 | 141M | INFORMATION DISPLAY STEERING WHEEL MOUNTED CONTROL COLUMN 3 SIGNAL | ?????
18 | 0.5 | 26N | ENGINE START/STOP + SIGNAL | ?????
19 | 0.5 | CANL | DIAGNOSTIC CAN L SIGNAL | ?????
20 | 0.5 | CANH | DIAGNOSTIC CAN H SIGNAL | ?????
22 | 0.5 | 26M | ENGINE RUNNING WARNING LIGHT CONTROL | ?????
24 | 0.3 | SP16 | PROTECTED + ACCESSORIES FEED / ACCESSORIES FEED FUSE SUPPLY | ?????
26 | 0.3 | 26LB | COLUMN STATUS SIGNAL 1 | ?????
27 | 0.3 | 26LC | COLUMN STATUS SIGNAL 2 | ?????
28 | 0.3 | 65Q | STOP SWITCH SIGNAL 2 | ?????
31 | 0.3 | 38FC | PASSENGER COMPARTMENT FAN CONTROL > RELAY | ?????
32 | 0.3 | 26HB | RADIO FREQUENCY UNIT SUPPLY | ?????
34 | 0.3 | 20M | DOOR LOCKING LED | ?????
35 | 0.3 | 26I | + STEERING COLUMN LOCK | ?????
36 | 0.3 | 141K | INFORMATION DISPLAY STEERING WHEEL MOUNTED CONTROL COLUMN 1 SIGNAL | ?????
37 | 0.3 | 141N | INFORMATION DISPLAY STEERING WHEEL MOUNTED CONTROL COLUMN 4 SIGNAL | ?????
38 | 0.3 | 141L | INFORMATION DISPLAY STEERING WHEEL MOUNTED CONTROL COLUMN 2 SIGNAL | ?????
39 | 0.5 | 64Q | FLASHER UNIT TIMER - CONTROL | ?????
40 | 0.3 | 26LA | PASSENGER COMPARTMENT COMMUNICATION SIGNAL/COLUMN LOCK | ?????