24342AX117
1	0.5	36C	REAR SCREEN WIPER PARK POSITION SWITCH - SIGNAL	?????
6	0.3	64Q	FLASHER UNIT TIMER - CONTROL	?????
7	0.5	BP10	PROTECTED + BATTERY FEED > DIAGNOSTIC SOCKET	?????
18	0.5	80FG	CENTRAL ELECTRICAL UNIT SIGNAL CODE / UCH COMPUTER CONTROL	?????
19	0.3	67A	HORN + CONTROL	?????
