24341AR443
1	0.85	34E	RIGHT HAND FRONT LOUDSPEAKER + SIGNAL	?????
2	0.85	34G	LEFT HAND FRONT LOUDSPEAKER + SIGNAL	?????
3	1.2	A1	+ AFTER IGNITION ELECTRIC WINDOW FUSE > RELAY	?????
4	1.2	20AR	DEADLOCKING MOTOR CONTROL	?????
5	1.2	20BD	OPEN FRONT/REAR PASSENGER DOORS MOTOR CONTROL	?????
6	1.2	23K	LEFT HAND REAR ELECTRIC WINDOW CONTROL 2 	?????
7	1.2	36A	REAR WIPER + CONTROL	?????
8	0.85	34F	RIGHT HAND FRONT LOUDSPEAKER - SIGNAL	?????
9	0.85	34H	LEFT HAND FRONT LOUDSPEAKER - SIGNAL	?????
10	1.2	15LP	PROTECTED HEATED REAR SCREEN + CONTROL	?????
11	1.2	BP48	PROTECTED + BATTERY FEED > ELECTRIC WINDOW	?????
12	1.2	A1	+ AFTER IGNITION ELECTRIC WINDOW FUSE > RELAY	?????
13	1.2	20D	ELECTRIC DOOR LOCKS CLOSE + CONTROL	?????
14	2.0	AP45	+ AFTER IGNITION FEED PROTECTED BY FUSE FOR PASSENGER COMPARTMENT FUNCTIONS	?????
15	1.2	BP48	PROTECTED + BATTERY FEED > ELECTRIC WINDOW	?????
16	1.2	23J	LEFT HAND REAR ELECTRIC WINDOW CONTROL 1 	?????
