| ENGINE WIRING
M9R/BVM6

#### 120
INJECTION COMPUTER
TR4X4/CA01,CA02/M9R830,M9R832

K2 | 0.5 | 3ABT | - TURBO UPSTREAM TEMPERATURE SENSOR | ?????
L2 | 2.0 | 3KW | INJECTOR 1 CONTROL | ?????
M2 | 2.0 | 3CR | INJECTOR 1 - CONTROL | ?????
A3 | 0.5 | 3FJ | INJECTION COMPUTER SENSOR - | ?????
C3 | 0.5 | 3XT | -PARTICLE FILTER UPSTREAM TEMPERATURE SENSOR | ?????
D3 | 0.5 | 38U | RHEOSTAT CURSOR | ?????
E3 | 0.5 | 38X | REFRIGERANT GAS PRESSURE SENSOR SIGNAL | ?????
F3 | 0.5 | 3TD | PARTICLE FILTER UPSTREAM TEMPERATURE SENSOR SIGNAL | ?????
G3 | 0.5 | 3XU | -PARTICLE FILTER DOWNSTREAM TEMPERATURE SENSOR | ?????
H3 | 0.5 | 3TG | PARTICLE FILTER DOWNSTREAM TEMPERATURE SENSOR SIGNAL | ?????
L3 | 2.0 | 3KX | INJECTOR 2 CONTROL | ?????
M3 | 2.0 | 3CS | INJECTOR 2 - CONTROL | ?????
A4 | 0.5 | 3CQ | CAMSHAFT SENSOR SIGNAL | ?????
D4 | 0.5 | 3GC | EGR SENSOR + | ?????
E4 | 0.5 | 3EL | EGR POTENTIOMETER + SIGNAL | ?????
F4 | 0.5 | 3C | COOLANT TEMPERATURE SENSOR + SIGNAL | ?????
G4 | 0.5 | 3JK | COOLANT TEMPERATURE - | ?????
H4 | 0.5 | 3MY | TURBOCHARGER PRESSURE SENSOR SIGNAL | ?????
J4 | 0.5 | 3MZ | - TURBOCHARGER PRESSURE SENSOR | ?????
K4 | 0.5 | 3AAS | UPSTREAM DIESEL OXYGEN SENSOR HEATING-CONTROL | ?????
L4 | 2.0 | 3KY | INJECTOR 3 CONTROL | ?????
M4 | 2.0 | 3CT | INJECTOR 3 - CONTROL | ?????
B1 | 0.5 | 38Y | REFRIGERANT GAS PRESSURE SENSOR + | ?????
C1 | 0.5 | 3AAQ | +PARTICLE FILTER DIFFERENTIAL PRESSURE SENSOR | ?????
D1 | 0.5 | 3JM | EGR SOLENOID VALVE - | ?????
E1 | 0.5 | 3LX | RAIL FUEL PRESSURE SENSOR + | ?????
F1 | 0.5 | 3MX | +5V TURBOCHARGER PRESSURE SENSOR | ?????
G1 | 0.5 | 3LQ | TURBOCHARGER PRESSURE SENSOR + | ?????
H1 | 0.5 | 3LN | TURBOCHARGER PRESSURE SENSOR - | ?????
K1 | 0.5 | 3FJ | INJECTION COMPUTER SENSOR - | ?????
L1 | 2.0 | 3KZ | INJECTOR 4 CONTROL | ?????
M1 | 2.0 | 3CU | INJECTOR 4 - CONTROL | ?????
B2 | 0.5 | 3TM | -PARTICLE FILTER DIFFERENTIAL PRESSURE SENSOR | ?????
C2 | 0.5 | 3TL | PARTICLE FILTER DIFFERENTIAL PRESSURE SIGNAL | ?????
D2 | 0.5 | 3LZ | RAIL FUEL PRESSURE SENSOR - | ?????
E2 | 0.5 | 3LY | RAIL FUEL PRESSURE SENSOR + SIGNAL | ?????
F2 | 0.5 | 3FAB | FUEL TEMPERATURE + SIGNAL | ?????
G2 | 0.5 | 3LD | FUEL TEMPERATURE SENSOR - | ?????
H2 | 0.5 | 3LP | TURBOCHARGER PRESSURE SENSOR + SIGNAL | ?????
J2 | 0.5 | 3ABS | TURBO UPSTREAM TEMPERATURE SENSOR + SIGNAL | ?????