| DASHBOARD WIRING
H45/DD

#### 325
RADIO SATELLITE CONTROL
FPAUTO/RDAVAR/SOP03/RETRCR/LVILVI/RAD03/BVA6/BVVR

1 | 0.5 | 34AS | RADIO SATELLITE IN0 SIGNAL | ?????
2 | 0.5 | 34AT | RADIO SATELLITE IN1 SIGNAL | ?????
3 | 0.5 | 34AU | RADIO SATELLITE IN2 SIGNAL | ?????
4 | 0.5 | 34AR | RADIO SATELLITE SIGNAL L2 | ?????
5 | 0.5 | 34AQ | RADIO SATELLITE SIGNAL L1 | ?????
6 | 0.5 | 34AP | RADIO SATELLITE SIGNAL L0 | ?????
7 | 0.5 | 34AO | RADIO SATELLITE L3 (LINE 3) SIGNAL | ?????