| CONNECTION
ANY TYPE

#### R455
DASHBOARD/LEFT REAR 5
H45/DG FPAUTO/RDAVAR/SOP03/RETRCR/LVILVI/RAD05/BVM6

2 | 0.5 | 34A | LEFT HAND REAR LOUDSPEAKER + SIGNAL | ?????
3 | 1.2 | A1 | + AFTER IGNITION ELECTRIC WINDOW FUSE > RELAY | ?????
4 | 0.5 | 20DE | PASSENGER DOOR LOCKING SIGNAL | ?????
5 | 1.2 | 20BD | OPEN FRONT/REAR PASSENGER DOORS MOTOR CONTROL | ?????
6 | 1.2 | 21ZB | WINDOW WINDER THERMAL PROTECTION SIGNAL | ?????
7 | 1.2 | 36A | REAR WIPER + CONTROL | ?????
9 | 0.5 | 34B | LEFT HAND REAR LOUDSPEAKER - SIGNAL | ?????
10 | 1.2 | 15LP | PROTECTED HEATED REAR SCREEN + CONTROL | ?????
11 | 1.2 | BP48 | PROTECTED + BATTERY FEED > ELECTRIC WINDOW | ?????
12 | 1.2 | A1 | + AFTER IGNITION ELECTRIC WINDOW FUSE > RELAY | ?????
13 | 1.2 | 20D | ELECTRIC DOOR LOCKS CLOSE + CONTROL | ?????
15 | 1.2 | BP48 | PROTECTED + BATTERY FEED > ELECTRIC WINDOW | ?????
16 | 0.3 | 23X | REAR LEFT-HAND ANTI-PINCH WINDOW WINDER SERIES SIGNAL | ?????