| CONNECTION
ANY TYPE

#### R323
SEAT / RIGHT-HAND SEAT ELECTRICAL FUNCTIONS
H45/DD TR4X4,TR4X2/NINAV1

1 | 0.3 | LP | PROTECTED + SIDE LIGHT FEED | ?????
2 | 0.3 | MZT | RIGHT-HAND REAR ELECTRIC EARTH ARRANGEMENT | ?????
4 | 1.2 | 79A | HEATED SEAT + CONTROL | ?????
5 | 1.2 | MZT | RIGHT-HAND REAR ELECTRIC EARTH ARRANGEMENT | ?????
6 | 0.5 | MZT | RIGHT-HAND REAR ELECTRIC EARTH ARRANGEMENT | ?????
7 | 0.5 | 60EH | FRONT RIGHT-HAND SEAT BELT SWITCH SIGNAL | ?????
8 | 1.2 | BP48 | PROTECTED + BATTERY FEED > ELECTRIC WINDOW | ?????