| FRONT WIRING
H45/BVVR/2TR

#### 1615
INTERNAL COMBUSTION ENGINE RUNNING + RELAY
DG/TR4X2/SSESP/NINAV4/RAD04,RAD05,RAD07

1 | 0.3 | MZR | FRONT SIDE MEMBER ELECTRIC EARTH ARRANGEMENT | ?????
2 | 0.5 | AP44 | POWER ASSISTED STEERING ECU + AFTER IGNITION FEED FUSE PROTECTION | ?????
3 | 3.0 | 38JS | CONTROL 1 REAR DISTRIBUTION MOTOR | ?????
4 | 1.2 | 79A | HEATED SEAT + CONTROL | ?????
5 | 1.2 | BP1B | + BATTERY PROTECTED > HEATED SEATS | ?????
6 | 3.0 | BP74 | PROTECTED + BATTERY FEED PASSENGER COMPARTMENT FAN FUSE | ?????