| FRONT WIRING
H45/BVVR/2TR

#### 597
ENGINE AND RELAY FUSE BOX
DD/TR4X4/ASRES2/LAVPH/NINAV1,NINAV2/RAD01,RAD02,RAD03

1 | 8.0 | BP7 | PROTECTED + BATTERY FEED > FAN FUSE 1 | ?????
2 | 3.0 | BP1Q | PROTECTED + BATTERY FEED/PASSENGER COMPARTMENT STARTING AND AFTER IGNITION | ?????
3 | 3.0 | BP73 | PROTECTED + BATTERY FEED FAN FUSE | ?????
4 | 3.0 | BP71 | PROTECTED + BATTERY FEED > FAN FUSE 2 | ?????
5 | 3.0 | BP7 | PROTECTED + BATTERY FEED > FAN FUSE 1 | ?????
6 | 3.0 | BP48 | PROTECTED + BATTERY FEED > ELECTRIC WINDOW | ?????
7 | 0.85 | BP26 | CARPHONE PROTECTED + BATTERY FEED | ?????
8 | 3.0 | BP89 | AUTOMATIC PARKING BRAKE FUSE PROTECTED + BATTERY FEED | ?????
9 | 3.0 | BP74 | PROTECTED + BATTERY FEED PASSENGER COMPARTMENT FAN FUSE | ?????
10 | 0.5 | BP42 | PROTECTED + BATTERY FEED > AUTOMATIC TRANSMISSION COMPUTER | ?????
11 | 8.0 | BP1C | + BATTERY PROTECTED > PROTECTION AND SWITCHING UNIT | ?????
12 | 8.0 | BP81 | PROTECTED + BATTERY FEED > ELECTRIC POWER-ASSISTED STEERING | ?????
13 | 1.2 | BP20 | PROTECTED + BATTERY FEED HEADLIGHT WASHERS | ?????
14 | 3.0 | BP8 | PROTECTED + BATTERY FEED > ANTI-LOCK BRAKING SYSTEM MOTOR | ?????
15 | 3.0 | BP1S | PROTECTED + BATTERY FEED / ENGINE INTER-CONNECTION UNIT SHUNT | ?????
16 | 3.0 | BP14 | PROTECTED + BATTERY FEED > ABS | ?????
17 | 0.5 | BPA4 | + BATTERY HORN PROTECTED FEED | ?????
20 | 1.2 | BP1B | + BATTERY PROTECTED > HEATED SEATS | ?????
21 | 0.5 | BPA4 | + BATTERY HORN PROTECTED FEED | ?????
22 | 0.5 | 67G | ELECTRIC CONTROL UNIT > AUDIBLE WARNING ACTIVATION SIGNAL | ?????
23 | 0.5 | 67E | + AUDIBLE WARNING RELAYED PROTECTED SUPPLY | ?????
24 | 3.0 | BP1S | PROTECTED + BATTERY FEED / ENGINE INTER-CONNECTION UNIT SHUNT | ?????
25 | 3.0 | BP7 | PROTECTED + BATTERY FEED > FAN FUSE 1 | ?????