| CONNECTION
ANY TYPE

#### R4
DASHBOARD/PASSENGER'S DOOR CONNECTION
H45/DD FMMANU,FPAUTO/RDAVAR/SOP01/RETRCR/LVILVE/NINAV1/BVM6

8 | 0.5 | 15RP | PROTECTED HEATED REAR VIEW MIRROR + CONTROL | F049
9 | 0.5 | 40E | REAR VIEW MIRROR MOTOR COMMON | F049
10 | 0.5 | 40A | DRIVER'S REAR VIEW MIRROR RIGHT>LEFT CONTROL | F049
16 | 0.5 | 34H | LEFT HAND FRONT LOUDSPEAKER - SIGNAL | F049
17 | 0.5 | 34G | LEFT HAND FRONT LOUDSPEAKER + SIGNAL | F049
20 | 0.5 | 13C | INTERIOR LIGHT - CONTROL | F049
21 | 0.5 | BPT | PROTECTED + BATTERY FEED TIMER | F049
22 | 0.5 | 40W | REAR-VIEW MIRROR FOLD IN CONTROL | F049
23 | 0.5 | 40X | REAR-VIEW MIRROR FOLD OUT CONTROL | F049
24 | 0.5 | 40C | DRIVER'S REAR VIEW MIRROR UP/DOWN CONTROL | F049