| DASHBOARD WIRING
H45/DD

#### 989
DISCHARGE BULB COMPUTER
FMMANU,FPAUTO/RDAVAR/SOP01/RETRCR/LVILVE/RAD01,RAD02/BVM6

1 | 0.5 | MZQ | DASHBOARD ELECTRIC EARTH ARRANGEMENT | ?????
2 | 0.5 | CPG | PROTECTED LEFT HAND DIPPED BEAM HEADLIGHT + | ?????
3 | 0.5 | CANH | DIAGNOSTIC CAN H SIGNAL | ?????
4 | 0.5 | AP44 | POWER ASSISTED STEERING ECU + AFTER IGNITION FEED FUSE PROTECTION | ?????
5 | 0.5 | CPD | PROTECTED RIGHT HAND DIPPED BEAM HEADLIGHT + | ?????
7 | 0.5 | BP10 | PROTECTED + BATTERY FEED > DIAGNOSTIC SOCKET | ?????
8 | 0.5 | CANL | DIAGNOSTIC CAN L SIGNAL | ?????