| CONNECTION
ANY TYPE

#### R374
REAR LEFT-HAND WIRING / FRONT WIRING HARNESS CONNECTION
H45/BVM6/M9R DG/TR4X4/ASRES2/NINAV4/RAD04,RAD05,RAD07

1 | 0.5 | 35D | FRONT LEFT-HAND INTERIOR PARKING PARKING PROXIMITY DETECTOR SENSOR 2 SIGNAL | F049
2 | 0.5 | 35G | FRONT LEFT-HAND EXTERIOR PARKING PARKING PROXIMITY DETECTOR SENSOR 1 SIGNAL | F049
3 | 0.5 | 35A | FRONT PARKING PROXIMITY DETECTOR SENSOR + FEED | F049
4 | 0.5 | 4S | RIGHT HAND REAR WHEEL SENSOR SIGNAL | F049
5 | 0.5 | 4G | LEFT HAND REAR WHEEL SENSOR SIGNAL | F049
7 | 0.5 | 150L | CLUTCH - SENSOR | F049
10 | 0.5 | 35B | FRONT PARKING PROXIMITY DETECTOR SENSOR - FEED | F049
11 | 0.5 | 35C | FRONT RIGHT-HAND INTERIOR PARKING PARKING PROXIMITY DETECTOR SENSOR 3 SIGNAL | F049
12 | 0.5 | 35H | FRONT RIGHT-HAND EXTERIOR PARKING PARKING PROXIMITY DETECTOR SENSOR 4 SIGNAL | F049
13 | 0.5 | 4T | RIGHT HAND REAR WHEEL SENSOR + | F049
14 | 0.5 | 4H | LEFT HAND REAR WHEEL SENSOR + | F049
15 | 0.5 | CANL | DIAGNOSTIC CAN L SIGNAL | F049
16 | 0.5 | CANH | DIAGNOSTIC CAN H SIGNAL | F049
18 | 0.5 | 150K | CLUTCH SENSOR SIGNAL | F049
19 | 0.5 | 150Q | CLUTCH SENSOR + | F049
20 | 0.5 | BP26 | CARPHONE PROTECTED + BATTERY FEED | F049