| CONNECTION
ANY TYPE

#### R374
REAR LEFT-HAND WIRING / FRONT WIRING HARNESS CONNECTION
H45/DG TR4X4/NINAV2,NINAV4/RAD03,RAD07

1 | 0.5 | 35D | FRONT LEFT-HAND INTERIOR PARKING PARKING PROXIMITY DETECTOR SENSOR 2 SIGNAL | M049
2 | 0.5 | 35G | FRONT LEFT-HAND EXTERIOR PARKING PARKING PROXIMITY DETECTOR SENSOR 1 SIGNAL | M049
3 | 0.5 | 35A | FRONT PARKING PROXIMITY DETECTOR SENSOR + FEED | M049
4 | 0.5 | 4S | RIGHT HAND REAR WHEEL SENSOR SIGNAL | M049
5 | 0.5 | 4G | LEFT HAND REAR WHEEL SENSOR SIGNAL | M049
7 | 0.5 | 150L | CLUTCH - SENSOR | M049
8 | 0.5 | 67G | ELECTRIC CONTROL UNIT > AUDIBLE WARNING ACTIVATION SIGNAL | M049
10 | 0.5 | 35B | FRONT PARKING PROXIMITY DETECTOR SENSOR - FEED | M049
11 | 0.5 | 35C | FRONT RIGHT-HAND INTERIOR PARKING PARKING PROXIMITY DETECTOR SENSOR 3 SIGNAL | M049
12 | 0.5 | 35H | FRONT RIGHT-HAND EXTERIOR PARKING PARKING PROXIMITY DETECTOR SENSOR 4 SIGNAL | M049
13 | 0.5 | 4T | RIGHT HAND REAR WHEEL SENSOR + | M049
14 | 0.5 | 4H | LEFT HAND REAR WHEEL SENSOR + | M049
15 | 0.5 | CANL | DIAGNOSTIC CAN L SIGNAL | M049
16 | 0.5 | CANH | DIAGNOSTIC CAN H SIGNAL | M049
18 | 0.5 | 150K | CLUTCH SENSOR SIGNAL | M049
19 | 0.5 | 150Q | CLUTCH SENSOR + | M049