243414M463
1	0.5	79FB	HEATED SEAT WARNING LIGHT CONTROL, HIGH POSITION	M004
2	0.5	79FA	HEATED SEAT WARNING LIGHT CONTROL, LOW POSITION	M004
3	0.5	BPT	PROTECTED + BATTERY FEED TIMER	M004
4	0.5	CANH	DIAGNOSTIC CAN H SIGNAL 	M004
5	0.5	107E	RADIO SOUND CUT-OFF SIGNAL FOR TELEPHONE	M004
6	0.5	TB45	RADIO SOCKET AUXILIARY SOCKET INPUT SHIELDED CABLE	M004
7	0.5	4CX	LATERAL ACCELERATION SENSOR SIGNAL	M004
8	0.5	4CV	YAW SENSOR REFERENCE SIGNAL (DIRECTIONAL STABILITY)	M004
9	0.5	3NAB	TANK PRESSURE SENSOR SIGNAL	M004
10	0.3	LP	PROTECTED + SIDE LIGHT FEED	M004
11	0.5	9P	PROTECTED REAR FOG LIGHTS + CONTROL	M004
12	0.5	34HU	MULTIMEDIA WAKE-UP SIGNAL	M004
13	0.5	13C	INTERIOR LIGHT - CONTROL	M004
14	0.5	CANL	DIAGNOSTIC CAN L SIGNAL 	M004
15	0.5	AP5	PROTECTED + AFTER IGNITION ANTI-LOCK BRAKING SYSTEM FUSE	M004
17	0.5	4DS	- YAW SENSOR	M004
18	0.5	4CW	YAW SENSOR SIGNAL (DIRECTIONAL STABILITY)	M004
19	0.5	41B	FUEL LEVEL  -	M004
20	0.5	41A	FUEL LEVEL SENDER + SIGNAL	M004
