| CONNECTION
ANY TYPE

#### R13
LEFT REAR/LEFT-HAND REAR DOOR CONNECTION
H45/DD TR4X2/RAD03/NINAV2

2 | 0.5 | BPT | PROTECTED + BATTERY FEED TIMER | F009
3 | 0.5 | 13C | INTERIOR LIGHT - CONTROL | F009
4 | 0.85 | 34A | LEFT HAND REAR LOUDSPEAKER + SIGNAL | F009
5 | 0.85 | 34B | LEFT HAND REAR LOUDSPEAKER - SIGNAL | F009
6 | 0.3 | 26AG | KEYLESS VEHICLE DRIVER'S SIDE REAR DOOR EXTERNAL AERIAL A SIGNAL | F009
7 | 0.3 | 26AH | KEYLESS VEHICLE DRIVER'S SIDE REAR DOOR EXTERNAL AERIAL B SIGNAL | F009
8 | 0.3 | 26CJ | DRIVER'S REAR DOOR SWITCH/LOCKING SIGNAL | F009
10 | 0.3 | 26P | DOOR HANDLE INFRARED SENSOR + | F009
11 | 1.2 | 23K | LEFT HAND REAR ELECTRIC WINDOW CONTROL 2 | ?????
12 | 1.2 | 23J | LEFT HAND REAR ELECTRIC WINDOW CONTROL 1 | ?????
13 | 1.2 | A1 | + AFTER IGNITION ELECTRIC WINDOW FUSE > RELAY | ?????
14 | 1.2 | MZS | LEFT-HAND REAR ELECTRIC EARTH ARRANGEMENT | ?????
15 | 1.2 | 20BD | OPEN FRONT/REAR PASSENGER DOORS MOTOR CONTROL | ?????
16 | 1.2 | 20D | ELECTRIC DOOR LOCKS CLOSE + CONTROL | ?????
17 | 1.2 | 20AR | DEADLOCKING MOTOR CONTROL | ?????
18 | 0.3 | 26S | DRIVER'S SIDE REAR HANDLE INFRARED SENSOR SIGNAL | ?????