| LEFT-HAND REAR WIRING
H45/DG

#### 756
AIR BAG/PRETENSIONER COMPUTER
TR4X4/RDAVAR/RAD02,RAD04,RAD05

1 | 0.5 | 60AS | - DRIVER'S SIDE THORAX AIR BAG CONTROL | F009
2 | 0.5 | 60BZ | DRIVER'S HEAD CURTAIN AIR BAG - CONTROL | F009
3 | 0.5 | 60AK | DRIVER'S LAP STRAP PRETENSIONER + CONTROL | F009
4 | 0.5 | 60BY | DRIVER'S HEAD CURTAIN AIR BAG + CONTROL | F009
6 | 0.5 | 60AR | DRIVER'S SIDE THORAX AIR BAG + CONTROL | F009
7 | 0.5 | 60E | DRIVER'S PRETENSIONER - SIGNAL | F009
8 | 0.5 | 60AL | DRIVER'S LAP STRAP PRETENSIONER - CONTROL | F009
9 | 0.5 | 60D | DRIVER'S PRETENSIONER + SIGNAL | F009
10 | 0.5 | 60KY | LEFT-HAND SIDE SATELLITE (AIRBAG) - SIGNAL | F009
11 | 0.5 | 60KX | LEFT-HAND SIDE SATELLITE (AIRBAG) + SIGNAL | F009
12 | 0.5 | NAU | LEFT HAND B-PILLAR ELECTRONIC EARTH | F009