| FRONT WIRING
H45/BVM6/M9R

#### 1337
SWITCHING PROTECTION UNIT
DG/TR4X4/ASRES2/LAVPH/NINAV1,NINAV2/RAD01,RAD02,RAD03

1 | 0.5 | 26Z | AUTOMATIC TRANSMISSION NEUTRAL + SIGNAL | ?????
2 | 0.5 | AP44 | POWER ASSISTED STEERING ECU + AFTER IGNITION FEED FUSE PROTECTION | ?????
3 | 0.5 | AP5 | PROTECTED + AFTER IGNITION ANTI-LOCK BRAKING SYSTEM FUSE | ?????
4 | 0.5 | 5HT | STARTER RELAY CONTROL | ?????
5 | 0.5 | LP | PROTECTED + SIDE LIGHT FEED | ?????
6 | 0.5 | LP | PROTECTED + SIDE LIGHT FEED | ?????
7 | 0.85 | RPD | RIGHT HAND PROTECTED MAIN BEAM HEADLIGHT + | ?????
8 | 0.5 | AP11 | PROTECTED + AFTER IGNITION REVERSING LIGHTS FUSE | ?????
9 | 1.2 | AP7 | PROTECTED + AFTER IGNITION WINDSCREEN WIPER FUSE | ?????
10 | 0.85 | AP28 | PROTECTED + AFTER IGNITION FUSE COOLING FAN ASSEMBLY | ?????
13 | 0.85 | CPD | PROTECTED RIGHT HAND DIPPED BEAM HEADLIGHT + | ?????
14 | 0.85 | CPG | PROTECTED LEFT HAND DIPPED BEAM HEADLIGHT + | ?????
15 | 0.5 | LP | PROTECTED + SIDE LIGHT FEED | ?????
16 | 0.85 | RPG | LEFT HAND PROTECTED MAIN BEAM HEADLIGHT + | ?????