| DASHBOARD WIRING
H45/DD

#### 645
PASSENGER COMPARTMENT COMPUTER
FMMANU,FPAUTO/RDAVAR/SOP01/RETRCR/LVILVE/NINAV1/BVM6

1 | 0.5 | BPT | PROTECTED + BATTERY FEED TIMER | ?????
2 | 1.2 | 20AR | DEADLOCKING MOTOR CONTROL | ?????
5 | 1.2 | 20D | ELECTRIC DOOR LOCKS CLOSE + CONTROL | ?????
6 | 1.2 | 20BC | DRIVER'S DOOR / FUEL FILLER FLAP UNLOCKING MOTOR CONTROL | ?????
7 | 1.2 | 20BD | OPEN FRONT/REAR PASSENGER DOORS MOTOR CONTROL | ?????
8 | 0.5 | BP6 | PROTECTED + BATTERY FEED > INTERIOR LIGHT | ?????
10 | 2.0 | MZQ | DASHBOARD ELECTRIC EARTH ARRANGEMENT | ?????
14 | 0.5 | 11S | RIGHT-HAND PROTECTED SIDE LIGHT +CONTROL | ?????
15 | 0.5 | 11T | LEFT-HAND PROTECTED SIDE LIGHT +CONTROL | ?????
16 | 0.5 | 13C | INTERIOR LIGHT - CONTROL | ?????