| DASHBOARD WIRING
H45/DD

#### 662
NAVIGATION COMPUTER
FPAUTO/RDAVAR/SOP03/RETRCR/LVILVI/NINAV2/BVM6

2 | 0.5 | 46BC | NAVIGATION CAN L SIGNAL | ?????
4 | 0.5 | 47F | VEHICLE SPEED SIGNAL | ?????
10 | 0.3 | 34HA | VIDEO DISPLAY CONTROL SIGNAL 2 | ?????
14 | 0.3 | 34DD | BLUE RGB VIDEO SIGNAL | ?????
15 | 0.3 | 34DB | RED RGB SIGNAL | ?????
18 | 0.5 | 46BB | NAVIGATION CAN H SIGNAL 1 | ?????
22 | 0.3 | LP | PROTECTED + SIDE LIGHT FEED | ?????
25 | 0.3 | TB30 | VIDEO CONTROL SHIELDED CABLE | ?????
26 | 0.3 | 34GZ | REMINDER | ?????
28 | 0.3 | TB32 | SHIELDED CABLE | ?????
29 | 0.3 | 34GU | RGB VIDEO SIGNAL EARTH (RED GREEN BLUE) | ?????
30 | 0.3 | 34DC | GREEN RGB VIDEO SIGNAL | ?????