| FRONT WIRING
H45/BVVR/2TR

#### 1410
TYRE PRESSURE MONITOR FRONT LEFT-HAND AERIAL
DD/TR4X4/ASRES2/LAVPH/NINAV1,NINAV2/RAD01,RAD02,RAD03

1 | 0.3 | 70BL | LEFT-HAND FRONT WHEEL AERIAL RECEIVER EARTH | F005E
2 | 0.3 | 70BG | LEFT-HAND FRONT WHEEL RADIO FREQUENCY AMPLITUDE SIGNAL | F005E
3 | 0.3 | 70BK | LEFT-HAND FRONT WHEEL AERIAL RECEIVER SIGNAL | F005E
4 | 0.3 | 70BE | LEFT-HAND FRONT WHEEL AERIAL RECEIVER + SUPPLY | F005E