| LEFT-HAND REAR WIRING
H45/DG

#### 1217
AUTOMATIC PARKING BRAKE ELECTRICAL UNIT
TR4X4/LADECH/NINAV2,NINAV4/RAD03,RAD07

A2 | 0.5 | CANL | DIAGNOSTIC CAN L SIGNAL | ?????
C2 | 0.5 | 150N | DYNAMIC BRAKE ACTUATOR SIGNAL | ?????
D2 | 0.5 | 150P | DYNAMIC BRAKE - ACTUATOR | ?????
E2 | 0.5 | 150L | CLUTCH - SENSOR | ?????
G2 | 2.0 | MZS | LEFT-HAND REAR ELECTRIC EARTH ARRANGEMENT | ?????
H2 | 2.0 | MZS | LEFT-HAND REAR ELECTRIC EARTH ARRANGEMENT | ?????
A3 | 0.5 | CANH | DIAGNOSTIC CAN H SIGNAL | ?????
C3 | 0.5 | 150D | STATIC LOCKING CONTROL | ?????
D3 | 0.5 | 150G | STATIC UNLOCKING CONTROL | ?????
E3 | 0.5 | 150K | CLUTCH SENSOR SIGNAL | ?????
C4 | 0.5 | 150H | LOCKING INDICATOR LIGHT CONTROL | ?????
E4 | 0.5 | 150Q | CLUTCH SENSOR + | ?????
G4 | 2.0 | BP89 | AUTOMATIC PARKING BRAKE FUSE PROTECTED + BATTERY FEED | ?????
H4 | 2.0 | BP89 | AUTOMATIC PARKING BRAKE FUSE PROTECTED + BATTERY FEED | ?????