| FRONT PASSENGER DOOR WIRING
H45/DG

#### 133
PASSENGER'S SIDE ELECTRIC WINDOW CONTROL
RET02,RET03/LVILVI/NINAV4/RAD03,RAD07

1 | 1.2 | 21ZA | WINDOW WINDER THERMAL PROTECTION SIGNAL 1 | ?????
2 | 1.2 | 22B | PASSENGER'S ELECTRIC WINDOW DOWN CONTROL | ?????
3 | 0.5 | MZQ | DASHBOARD ELECTRIC EARTH ARRANGEMENT | ?????
4 | 1.2 | A1 | + AFTER IGNITION ELECTRIC WINDOW FUSE > RELAY | ?????
7 | 1.2 | 22AA | PASSENGER ELECTRIC WINDOW RAISE/LOWER CONTROL | ?????
8 | 1.2 | 22A | PASSENGER'S ELECTRIC WINDOW UP CONTROL | ?????