| DASHBOARD WIRING
H45/DG

#### 260
PASSENGER COMPARTMENT FUSE BOX AND RELAY
FMMANU/SOP01/LVILVE/RAD01/BVM6

3 | 0.5 | 65A | BRAKE LIGHTS + CONTROL | ?????
4 | 0.3 | 15M | HEATED REAR SCREEN RELAY - CONTROL | ?????
5 | 0.3 | SP16 | PROTECTED + ACCESSORIES FEED / ACCESSORIES FEED FUSE SUPPLY | ?????
6 | 0.5 | BP10 | PROTECTED + BATTERY FEED > DIAGNOSTIC SOCKET | ?????
7 | 0.85 | SP4G | CIGARETTE LIGHTER PROTECTED + ACCESSORIES FEED | ?????
8 | 0.5 | LP | PROTECTED + SIDE LIGHT FEED | ?????
9 | 0.3 | BPA7 | BRAKE LIGHTS + BATTERY PROTECTED | ?????