| DASHBOARD WIRING
H45/DG

#### 247
INSTRUMENT PANEL
FPAUTO/RDAVAR/SOP03/RETRCR/LVILVI/NINAV4/BVA6,BVVR

1 | 0.5 | 79FB | HEATED SEAT WARNING LIGHT CONTROL, HIGH POSITION | ?????
3 | 0.3 | 87H | DRIVER'S 1st POSITION SWITCH - SIGNAL | ?????
4 | 0.5 | 47Y | DRIVING ASSISTANCE DISPLAY + CONTROL | ?????
5 | 0.3 | 47F | VEHICLE SPEED SIGNAL | ?????
5 | 0.5 | 47F | VEHICLE SPEED SIGNAL | ?????
6 | 0.3 | H47 | VEHICLE SPEED > SECONDARY SPEED SIGNAL | ?????
6 | 0.3 | H47 | VEHICLE SPEED > SECONDARY SPEED SIGNAL | ?????
7 | 0.5 | CANL | DIAGNOSTIC CAN L SIGNAL | ?????
8 | 0.5 | CANH | DIAGNOSTIC CAN H SIGNAL | ?????
11 | 0.3 | 87H | DRIVER'S 1st POSITION SWITCH - SIGNAL | ?????
13 | 0.5 | MZQ | DASHBOARD ELECTRIC EARTH ARRANGEMENT | ?????
14 | 0.5 | 32B | OIL LEVEL SENSOR SIGNAL 1 | ?????
16 | 0.5 | 79FA | HEATED SEAT WARNING LIGHT CONTROL, LOW POSITION | ?????