| CONNECTION
ANY TYPE

#### R12
RIGHT REAR/RIGHT-HAND REAR DOOR CONNECTION
H45 DG/LVILVE/NINAV4/RAD07

2 | 0.5 | BPT | PROTECTED + BATTERY FEED TIMER | L009
3 | 0.5 | 13C | INTERIOR LIGHT - CONTROL | L009
4 | 0.85 | 34C | RIGHT HAND REAR LOUDSPEAKER - SIGNAL | L009
5 | 0.85 | 34D | RIGHT HAND REAR LOUDSPEAKER + SIGNAL | L009
11 | 1.2 | 23H | RIGHT HAND REAR ELECTRIC WINDOW CONTROL 2 | ?????
12 | 1.2 | 23G | RIGHT HAND REAR ELECTRIC WINDOW CONTROL 1 | ?????
13 | 1.2 | A1 | + AFTER IGNITION ELECTRIC WINDOW FUSE > RELAY | ?????
14 | 1.2 | MZT | RIGHT-HAND REAR ELECTRIC EARTH ARRANGEMENT | ?????
15 | 1.2 | 20BD | OPEN FRONT/REAR PASSENGER DOORS MOTOR CONTROL | ?????
16 | 1.2 | 20D | ELECTRIC DOOR LOCKS CLOSE + CONTROL | ?????
17 | 0.5 | 20DE | PASSENGER DOOR LOCKING SIGNAL | ?????