| FRONT WIRING
H45/BVA6/M9R

#### 1410
TYRE PRESSURE MONITOR FRONT LEFT-HAND AERIAL
DG/TR4X4/SSESP/NINAV4/RAD04,RAD05,RAD07

1 | 0.3 | 70BL | LEFT-HAND FRONT WHEEL AERIAL RECEIVER EARTH | F005E
2 | 0.3 | 70BG | LEFT-HAND FRONT WHEEL RADIO FREQUENCY AMPLITUDE SIGNAL | F005E
3 | 0.3 | 70BK | LEFT-HAND FRONT WHEEL AERIAL RECEIVER SIGNAL | F005E
4 | 0.3 | 70BE | LEFT-HAND FRONT WHEEL AERIAL RECEIVER + SUPPLY | F005E