| DRIVER'S DOOR WIRING
H45/DG

#### 134
ELECTRIC REAR-VIEW MIRROR CONTROL
RET01,RET03/LVILVI/NINAV1/RAD01,RAD02,RAD04,RAD05

A4 | 0.5 | 40D | PASSENGER REAR VIEW MIRROR RIGHT>LEFT CONTROL | CB3X
B4 | 0.5 | 40A | DRIVER'S REAR VIEW MIRROR RIGHT>LEFT CONTROL | CB3X
A1 | 0.5 | 40E | REAR VIEW MIRROR MOTOR COMMON | CB3X
A2 | 0.5 | 40AA | REAR-VIEW MIRROR EARTH > REAR VIEW MIRROR ANTI-RETURN DIODE | CB3X
B2 | 0.5 | 40C | DRIVER'S REAR VIEW MIRROR UP/DOWN CONTROL | CB3X
A3 | 0.5 | 40B | PASSENGER REAR VIEW MIRROR UP/DOWN CONTROL | CB3X
B3 | 0.5 | SP2 | PROTECTED + ACCESSORIES > RADIO | CB3X