| LEFT-HAND REAR WIRING
H45/DD

#### 1876
SPEAKER (BASS SECTION)
TR4X4/LADECH/NINAV2/RAD03

1 | 0.5 | 34EH | SPEAKER + SIGNAL (BASS SECTION) | C426E
2 | 0.3 | 34EL | SPEAKER AMPLIFIER CONTROL (BASS SECTION) | C426E
3 | 2.0 | AP45 | + AFTER IGNITION FEED PROTECTED BY FUSE FOR PASSENGER COMPARTMENT FUNCTIONS | ?????
4 | 0.5 | 34EJ | SPEAKER - SIGNAL (BASS SECTION) | C426E
5 | 0.5 | TB38 | SPEAKER SHIELDED CABLE (BASS SECTION) | C426E
6 | 2.0 | MZS | LEFT-HAND REAR ELECTRIC EARTH ARRANGEMENT | ?????