| LEFT-HAND REAR WIRING
H45/DD

#### 1372
REAR HEIGHT SENSOR
TR4X4/RDAVAR/RAD02,RAD04,RAD05

2 | 0.5 | LP | PROTECTED + SIDE LIGHT FEED | ?????
3 | 0.3 | 47F | VEHICLE SPEED SIGNAL | ?????
4 | 0.5 | AP44 | POWER ASSISTED STEERING ECU + AFTER IGNITION FEED FUSE PROTECTION | ?????
5 | 0.5 | 103A | HEADLIGHT POSITION CONTROL | ?????
6 | 0.3 | HK | DIAGNOSTIC SIGNAL K | ?????
8 | 0.5 | MZS | LEFT-HAND REAR ELECTRIC EARTH ARRANGEMENT | ?????