| CONNECTION
ANY TYPE

#### R456
DRIVER'S DOOR WIRING/DASHBOARD WIRING CONNECTION 2
H45/DD FMMANU,FPAUTO/RDAVAR/SOP01/RETRCR/LVILVE/NINAV1/BVM6

1 | 1.2 | 23H | RIGHT HAND REAR ELECTRIC WINDOW CONTROL 2 | ?????
2 | 1.2 | 22A | PASSENGER'S ELECTRIC WINDOW UP CONTROL | ?????
3 | 1.2 | 22B | PASSENGER'S ELECTRIC WINDOW DOWN CONTROL | ?????
4 | 2.0 | A1 | + AFTER IGNITION ELECTRIC WINDOW FUSE > RELAY | ?????
5 | 2.0 | BP48 | PROTECTED + BATTERY FEED > ELECTRIC WINDOW | ?????
6 | 1.2 | 23J | LEFT HAND REAR ELECTRIC WINDOW CONTROL 1 | ?????
7 | 1.2 | 23K | LEFT HAND REAR ELECTRIC WINDOW CONTROL 2 | ?????
8 | 1.2 | 23G | RIGHT HAND REAR ELECTRIC WINDOW CONTROL 1 | ?????
9 | 1.2 | 20AR | DEADLOCKING MOTOR CONTROL | ?????
10 | 1.2 | 20D | ELECTRIC DOOR LOCKS CLOSE + CONTROL | ?????
11 | 1.2 | 20BC | DRIVER'S DOOR / FUEL FILLER FLAP UNLOCKING MOTOR CONTROL | ?????
12 | 1.2 | MZQ | DASHBOARD ELECTRIC EARTH ARRANGEMENT | ?????