| CONNECTION
ANY TYPE

#### R464
PEDALS/DASHBOARD 4
H45/BVM6/M9R DG/TR4X4/SSESP/NINAV4/RAD04,RAD05,RAD07

2 | 0.5 | 26Z | AUTOMATIC TRANSMISSION NEUTRAL + SIGNAL | ?????
4 | 0.3 | 38FC | PASSENGER COMPARTMENT FAN CONTROL > RELAY | ?????
5 | 0.3 | A5 | ENGINE AFTER IGNITION CONTROL RELAY | ?????
6 | 0.3 | 70BA | RIGHT-HAND FRONT WHEEL AERIAL RECEIVER + SUPPLY | ?????
7 | 0.3 | 70BB | RIGHT-HAND FRONT WHEEL RADIO FREQUENCY AMPLITUDE SIGNAL | ?????
8 | 0.3 | 70BE | LEFT-HAND FRONT WHEEL AERIAL RECEIVER + SUPPLY | ?????
9 | 0.3 | 70BG | LEFT-HAND FRONT WHEEL RADIO FREQUENCY AMPLITUDE SIGNAL | ?????
10 | 0.5 | APCB | + AFTER IGNITION PROTECTED / COLUMN LOCK FUSE CONTACT CLOSED AT REST | ?????
13 | 0.5 | 3WT | WATER IN DIESEL DETECTION SENSOR SIGNAL | ?????
14 | 0.5 | 5HT | STARTER RELAY CONTROL | ?????
15 | 0.5 | 26N | ENGINE START/STOP + SIGNAL | ?????
16 | 0.3 | 70BD | RIGHT-HAND FRONT WHEEL AERIAL RECEIVER EARTH | ?????
17 | 0.3 | 70BC | RIGHT-HAND FRONT WHEEL AERIAL RECEIVER SIGNAL | ?????
18 | 0.3 | 70BL | LEFT-HAND FRONT WHEEL AERIAL RECEIVER EARTH | ?????
19 | 0.3 | 70BK | LEFT-HAND FRONT WHEEL AERIAL RECEIVER SIGNAL | ?????
20 | 0.5 | 67G | ELECTRIC CONTROL UNIT > AUDIBLE WARNING ACTIVATION SIGNAL | ?????