| DRIVER'S DOOR WIRING
H45/DG

#### 132
DRIVER'S SIDE ELECTRIC WINDOW CONTROL
RET03/LVILVI/NINAV2/RAD03,RAD07

1 | 0.5 | 21C | ONE-TOUCH ELECTRIC WINDOW NORMAL UP - CONTROL | ?????
2 | 0.5 | 21E | ONE-TOUCH ELECTRIC WINDOW NORMAL DOWN - CONTROL | ?????
4 | 1.2 | 21ZA | WINDOW WINDER THERMAL PROTECTION SIGNAL 1 | ?????
5 | 1.2 | MZQ | DASHBOARD ELECTRIC EARTH ARRANGEMENT | ?????
6 | 0.5 | 21AA | DRIVER ELECTRIC WINDOW RAISE/LOWER CONTROL | ?????
8 | 0.3 | 23X | REAR LEFT-HAND ANTI-PINCH WINDOW WINDER SERIES SIGNAL | ?????
10 | 1.2 | A1 | + AFTER IGNITION ELECTRIC WINDOW FUSE > RELAY | ?????