| FRONT WIRING
H45/BVA6/M9R

#### 1337
SWITCHING PROTECTION UNIT
DG/TR4X4/ASRES2/LAVPH/NINAV1,NINAV2/RAD01,RAD02,RAD03,RAD04,RAD05,RAD07

1 | 0.5 | AP4 | PROTECTED + AFTER IGNITION AUTOMATIC TRANSMISSION FUSE | ?????
2 | 0.5 | 78H | DAY>NIGHT RELAY CONTROL | ?????
3 | 0.5 | 38JV | PASSENGER COMPARTMENT HEATING RESISTANCE CONTROL RELAY 2PASSENGER | ?????
5 | 0.5 | 49BA | FAN CONTROL RELAY 1 | ?????
6 | 0.5 | 38JU | PASSENGER COMPARTMENT HEATING RESISTANCE CONTROL RELAY 1 | ?????
8 | 0.3 | A5 | ENGINE AFTER IGNITION CONTROL RELAY | ?????
10 | 0.5 | 38JW | PASSENGER COMPARTMENT HEATING RESISTANCE CONTROL RELAY 3 | ?????
11 | 0.3 | 67G | ELECTRIC CONTROL UNIT > AUDIBLE WARNING ACTIVATION SIGNAL | ?????
12 | 0.5 | 39G | HEADLIGHT WASHERS RELAY 1 + CONTROL | ?????