| FRONT WIRING
H45/BVM6/M9R

#### 118
ANTI-LOCK BRAKING SYSTEM COMPUTER
DG/TR4X2/SSESP/NINAV1,NINAV2/RAD01,RAD02,RAD03

1 | 3.0 | BP8 | PROTECTED + BATTERY FEED > ANTI-LOCK BRAKING SYSTEM MOTOR | ?????
2 | 3.0 | BP14 | PROTECTED + BATTERY FEED > ABS | ?????
3 | 3.0 | MAH | ANTI-LOCK BRAKING SYSTEM ELECTRICAL EARTH | ?????
4 | 3.0 | MAH | ANTI-LOCK BRAKING SYSTEM ELECTRICAL EARTH | ?????
8 | 0.5 | 65A | BRAKE LIGHTS + CONTROL | F005E
9 | 0.5 | CANL | DIAGNOSTIC CAN L SIGNAL | F005E
11 | 0.5 | 4T | RIGHT HAND REAR WHEEL SENSOR + | F005E
12 | 0.5 | 4M | RIGHT HAND FRONT WHEEL SENSOR SIGNAL | F005E
15 | 0.5 | 4S | RIGHT HAND REAR WHEEL SENSOR SIGNAL | F005E
16 | 0.5 | AP5 | PROTECTED + AFTER IGNITION ANTI-LOCK BRAKING SYSTEM FUSE | F005E
21 | 0.5 | 4N | RIGHT HAND FRONT WHEEL SENSOR + | F005E
22 | 0.5 | CANH | DIAGNOSTIC CAN H SIGNAL | F005E
23 | 0.5 | 4E | LEFT HAND FRONT WHEEL SENSOR + | F005E
26 | 0.5 | 4H | LEFT HAND REAR WHEEL SENSOR + | F005E
27 | 0.5 | 4C | LEFT HAND FRONT WHEEL SENSOR SIGNAL | F005E
30 | 0.5 | 4G | LEFT HAND REAR WHEEL SENSOR SIGNAL | F005E