| CONNECTION
ANY TYPE

#### R462
PEDALS/DASHBOARD 2
H45/DD FPAUTO/RDAVAR/SOP03/RETRCR/LVILVI/NINAV2/BVM6

1 | 0.3 | 3PD | SPEED LIMITER ON/OFF CONTROL | M004
2 | 0.5 | MZT | RIGHT-HAND REAR ELECTRIC EARTH ARRANGEMENT | M004
3 | 0.5 | 4CX | LATERAL ACCELERATION SENSOR SIGNAL | ?????
3 | 0.5 | 4CX | LATERAL ACCELERATION SENSOR SIGNAL | ?????
4 | 0.5 | 4CV | YAW SENSOR REFERENCE SIGNAL (DIRECTIONAL STABILITY) | ?????
4 | 0.5 | 4CV | YAW SENSOR REFERENCE SIGNAL (DIRECTIONAL STABILITY) | ?????
5 | 0.5 | 4AQ | ELECTRONIC STABILITY PROGRAM ON/OFF SWITCH - CONTROL | M004
6 | 0.5 | 86D | DECLUTCH + SIGNAL | M004
7 | 0.5 | AP5 | PROTECTED + AFTER IGNITION ANTI-LOCK BRAKING SYSTEM FUSE | M004
8 | 0.5 | MZR | FRONT SIDE MEMBER ELECTRIC EARTH ARRANGEMENT | M004
9 | 0.5 | 32B | OIL LEVEL SENSOR SIGNAL 1 | M004
10 | 0.5 | 86M | CRUISE CONTROL PROGRAMMING RETURN SIGNAL | M004
11 | 0.3 | 3FX | CRUISE CONTROL ON>OFF - CONTROL | M004
12 | 0.5 | 86G | CRUISE CONTROL PROGRAMMING CONTROL | M004
13 | 0.5 | 4DS | - YAW SENSOR | ?????
13 | 0.5 | 4DS | - YAW SENSOR | ?????
14 | 0.5 | 4CW | YAW SENSOR SIGNAL (DIRECTIONAL STABILITY) | ?????
14 | 0.5 | 4CW | YAW SENSOR SIGNAL (DIRECTIONAL STABILITY) | ?????
15 | 0.5 | 4CZG | GRADIENT CONTROL (UP/DOWN) ON/OFF CONTROL | M004
16 | 0.5 | AP5 | PROTECTED + AFTER IGNITION ANTI-LOCK BRAKING SYSTEM FUSE | M004
17 | 0.5 | AP1C | PROTECTED + AFTER IGNITION FEED/4X4 COMPUTER | M004
18 | 0.5 | 4LA | ELECTRONIC STABILITY CONTROL/4X4 COMPUTER LIN SIGNAL | M004
19 | 0.5 | 115A | OIL TEMPERATURE SENSOR - SIGNAL | M004
20 | 0.5 | HK | DIAGNOSTIC SIGNAL K | M004