| DASHBOARD WIRING
H45/DG

#### 653
CLOCK/EXTERNAL TEMPERATURE/CARPHONE DISPLAY ASSEMBLY
FPAUTO/RDAVAR/SOP03/RETRCR/LVILVI/RAD07/BVA6,BVVR

1 | 0.5 | 34HY | MULTIMEDIA STOP/START CONTROL | ?????
2 | 0.5 | SP2 | PROTECTED + ACCESSORIES > RADIO | ?????
3 | 0.5 | BP26 | CARPHONE PROTECTED + BATTERY FEED | ?????
4 | 0.5 | 34AP | RADIO SATELLITE SIGNAL L0 | ?????
5 | 0.5 | 34AQ | RADIO SATELLITE SIGNAL L1 | ?????
6 | 0.5 | 34AR | RADIO SATELLITE SIGNAL L2 | ?????
7 | 0.5 | 34AO | RADIO SATELLITE L3 (LINE 3) SIGNAL | ?????
8 | 0.5 | 34AU | RADIO SATELLITE IN2 SIGNAL | ?????
9 | 0.5 | 34AT | RADIO SATELLITE IN1 SIGNAL | ?????
10 | 0.5 | 34AS | RADIO SATELLITE IN0 SIGNAL | ?????
11 | 0.5 | 34HU | MULTIMEDIA WAKE-UP SIGNAL | ?????
12 | 0.5 | MZQ | DASHBOARD ELECTRIC EARTH ARRANGEMENT | ?????
15 | 0.5 | 107X | DIAGNOSTIC SOCKET CANL MULTIMEDIA SIGNAL | ?????
16 | 0.5 | 107W | DIAGNOSTIC SOCKET CANH MULTIMEDIA SIGNAL | ?????
17 | 0.5 | CANL | DIAGNOSTIC CAN L SIGNAL | ?????
18 | 0.5 | CANH | DIAGNOSTIC CAN H SIGNAL | ?????