| CONNECTION
ANY TYPE

#### R3
DASHBOARD/DRIVER'S DOOR CONNECTION
H45/DG RET03/LVILVE/NINAV2/RAD03,RAD07

17 | 0.85 | 34G | LEFT HAND FRONT LOUDSPEAKER + SIGNAL | M049
20 | 0.5 | 13C | INTERIOR LIGHT - CONTROL | M049
21 | 0.5 | BPT | PROTECTED + BATTERY FEED TIMER | M049
22 | 0.5 | 40W | REAR-VIEW MIRROR FOLD IN CONTROL | M049
23 | 0.5 | 40X | REAR-VIEW MIRROR FOLD OUT CONTROL | M049
24 | 0.5 | 40B | PASSENGER REAR VIEW MIRROR UP/DOWN CONTROL | M049
8 | 0.5 | 15RP | PROTECTED HEATED REAR VIEW MIRROR + CONTROL | M049
9 | 0.5 | 40E | REAR VIEW MIRROR MOTOR COMMON | M049
10 | 0.5 | 40D | PASSENGER REAR VIEW MIRROR RIGHT>LEFT CONTROL | M049
11 | 0.5 | SP2 | PROTECTED + ACCESSORIES > RADIO | M049
16 | 0.85 | 34H | LEFT HAND FRONT LOUDSPEAKER - SIGNAL | M049