| CENTRAL COURTESY LIGHT WIRING
H45

#### 1978
LEVEL SENSOR (VEHICLE TILT)
DG/ALEVA/RETRCR/EQPT2,EQPT3

1 | 0.5 | 85AB | INSTRUMENT PANEL/RIDE HEIGHT SENSOR (COMPASS) SERIES CONNECTION EARTH | ?????
3 | 0.5 | 85AA | INSTRUMENT PANEL/RIDE HEIGHT SENSOR (COMPASS) SERIES CONNECTION + SIGNAL | ?????
4 | 0.5 | AP43 | PROTECED + AFTER IGNITION FUSE | ?????
5 | 0.5 | MZQ | DASHBOARD ELECTRIC EARTH ARRANGEMENT | ?????