| CONNECTION
ANY TYPE

#### R454
DASHBOARD/LEFT REAR 4
H45/DG TR4X2/SOP01/RAD02,RAD04,RAD05

1 | 0.5 | 36C | REAR SCREEN WIPER PARK POSITION SWITCH - SIGNAL | M004
6 | 0.3 | 64Q | FLASHER UNIT TIMER - CONTROL | M004
7 | 0.5 | BP10 | PROTECTED + BATTERY FEED > DIAGNOSTIC SOCKET | M004
18 | 0.5 | 80FG | CENTRAL ELECTRICAL UNIT SIGNAL CODE / UCH COMPUTER CONTROL | M004
19 | 0.3 | 67A | HORN + CONTROL | M004