| LEFT-HAND REAR WIRING
H45/DG

#### 1222
PARKING AID COMPUTER
TR4X4/RDAVAR/RAD02,RAD04,RAD05

1 | 0.5 | CANL | DIAGNOSTIC CAN L SIGNAL | CQ0A
2 | 0.5 | 35H | FRONT RIGHT-HAND EXTERIOR PARKING PARKING PROXIMITY DETECTOR SENSOR 4 SIGNAL | CQ0A
3 | 0.5 | 35G | FRONT LEFT-HAND EXTERIOR PARKING PARKING PROXIMITY DETECTOR SENSOR 1 SIGNAL | CQ0A
4 | 0.5 | 35C | FRONT RIGHT-HAND INTERIOR PARKING PARKING PROXIMITY DETECTOR SENSOR 3 SIGNAL | CQ0A
5 | 0.5 | 35D | FRONT LEFT-HAND INTERIOR PARKING PARKING PROXIMITY DETECTOR SENSOR 2 SIGNAL | CQ0A
7 | 0.5 | 35B | FRONT PARKING PROXIMITY DETECTOR SENSOR - FEED | CQ0A
8 | 0.5 | CANH | DIAGNOSTIC CAN H SIGNAL | CQ0A
11 | 0.5 | 35N | FRONT LOUDSPEAKER SIGNAL | CQ0A
12 | 0.5 | 35A | FRONT PARKING PROXIMITY DETECTOR SENSOR + FEED | CQ0A