| CONNECTION
ANY TYPE

#### R1
DASHBOARD/RIGHT REAR CONNECTION
H45/DG FPAUTO/RDAVAR/SOP03/RETRCR/LVILVI/RAD07/BVA6,BVVR

2 | 1.2 | 20BD | OPEN FRONT/REAR PASSENGER DOORS MOTOR CONTROL | F010
3 | 0.3 | 23X | REAR LEFT-HAND ANTI-PINCH WINDOW WINDER SERIES SIGNAL | ?????
4 | 1.2 | SP4A | ACCESSORIES SOCKET 2 PROTECTED + ACCESSORIES FEED | ?????
6 | 1.2 | 20D | ELECTRIC DOOR LOCKS CLOSE + CONTROL | ?????
7 | 1.2 | 21ZB | WINDOW WINDER THERMAL PROTECTION SIGNAL | ?????
8 | 1.2 | A1 | + AFTER IGNITION ELECTRIC WINDOW FUSE > RELAY | ?????
9 | 1.2 | 3N | FUEL PUMP + | ?????
12 | 0.85 | BP26 | CARPHONE PROTECTED + BATTERY FEED | F010
14 | 0.5 | 64D | RIGHT HAND TURN SIGNAL LIGHTS CONTROL | ?????
15 | 0.5 | 107X | DIAGNOSTIC SOCKET CANL MULTIMEDIA SIGNAL | ?????
16 | 0.5 | 107W | DIAGNOSTIC SOCKET CANH MULTIMEDIA SIGNAL | ?????
17 | 1.2 | 79A | HEATED SEAT + CONTROL | ?????
18 | 0.5 | 20DE | PASSENGER DOOR LOCKING SIGNAL | ?????
19 | 3.0 | 38JS | CONTROL 1 REAR DISTRIBUTION MOTOR | ?????