| DASHBOARD WIRING
H45/DG

#### 261
RADIO
FMMANU/SOP01/LVILVE/RAD01/BVM6

B3 | 0.5 | 34EV | RIGHT-HAND FRONT SPEAKER + SIGNAL (TWEETER) | CT2F
A4 | 0.85 | BP26 | CARPHONE PROTECTED + BATTERY FEED | CT2F
B4 | 0.5 | 34EW | RIGHT-HAND FRONT SPEAKER - SIGNAL (TWEETER) | CT2F
B5 | 0.5 | 34G | LEFT HAND FRONT LOUDSPEAKER + SIGNAL | CT2F
B6 | 0.5 | 34H | LEFT HAND FRONT LOUDSPEAKER - SIGNAL | CT2F
A8 | 0.85 | MT | RADIO ELECTRICAL EARTH | CT2F